## GstVc1Parser GstVc1Parser — Convenience library for parsing vc1 video bitstream. |

## Functions

GstVC1ParserResult | gst_vc1_identify_next_bdu ()
GstVC1ParserResult | gst_vc1_parse_sequence_header ()
GstVC1ParserResult | gst_vc1_parse_sequence_layer ()
GstVC1ParserResult | gst_vc1_parse_sequence_header_struct_a ()
GstVC1ParserResult | gst_vc1_parse_sequence_header_struct_b ()
GstVC1ParserResult | gst_vc1_parse_sequence_header_struct_c ()
GstVC1ParserResult | gst_vc1_parse_entry_point_header ()
GstVC1ParserResult | gst_vc1_parse_frame_header ()
GstVC1BitPlanes * | gst_vc1_bitplanes_new ()
void | gst_vc1_bitplanes_free ()
void | gst_vc1_bitplanes_free_1 ()
gboolean | gst_vc1_bitplanes_ensure_size ()

## Types and Values

#define | MAX_HRD_NUM_LEAKY_BUCKETS
#define | GST_VC1_BFRACTION_BASIS
enum | GstVC1StartCode
enum | GstVC1Profile
enum | GstVC1ParserResult
enum | GstVC1PictureType
enum | GstVC1Level
enum | GstVC1QuantizerSpec
enum | GstVC1DQProfile
enum | GstVC1Condover
enum | GstVC1MvMode
struct | GstVC1SeqHdr
struct | GstVC1AdvancedSeqHdr
struct | GstVC1SeqLayer
struct | GstVC1SeqStructA
struct | GstVC1SeqStructB
struct | GstVC1SeqStructC
struct | GstVC1HrdParam
struct | GstVC1EntryPointHdr
struct | GstVC1FrameHdr
struct | GstVC1PicAdvanced
struct | GstVC1PicSimpleMain
| GstVC1Picture
struct | GstVC1VopDquant
struct | GstVC1BDU

## Includes

    #include <gst/codecparsers/gstvc1parser.h>

## Description

For more details about the structures, look at the smpte specifications (S421m-2006.pdf).

## Functions

### gst_vc1_identify_next_bdu ()

    GstVC1ParserResult
    gst_vc1_identify_next_bdu (const guint8 *data,
                               gsize size,
                               GstVC1BDU *bdu);

Parses `data` and fills `bdu` fields

#### Parameters

data | The data to parse |
size | the size of `data` |
bdu | The GstVC1BDU where to store parsed bdu headers. | [out]

#### Returns

a GstVC1ParserResult

### gst_vc1_parse_sequence_header ()

    GstVC1ParserResult
    gst_vc1_parse_sequence_header (const guint8 *data,
                                   gsize size,
                                   GstVC1SeqHdr *seqhdr);

Parses `data` , and fills `seqhdr` fields.

#### Parameters

data | The data to parse |
size | the size of `data` |
seqhdr | The GstVC1SeqHdr to set. |

#### Returns

a GstVC1ParserResult

### gst_vc1_parse_sequence_layer ()

    GstVC1ParserResult
    gst_vc1_parse_sequence_layer (const guint8 *data,
                                  gsize size,
                                  GstVC1SeqLayer *seqlayer);

Parses `data` , and fills `seqlayer` fields.

#### Parameters

data | The data to parse |
size | the size of `data` |
seqlayer | The GstVC1SeqLayer to set. |

#### Returns

a GstVC1ParserResult

### gst_vc1_parse_sequence_header_struct_a ()

    GstVC1ParserResult
    gst_vc1_parse_sequence_header_struct_a
                                   (const guint8 *data,
                                    gsize size,
                                    GstVC1SeqStructA *structa);

Parses `data` , and fills `structa` fields.

#### Parameters

data | The data to parse |
size | the size of `data` |
structa | The GstVC1SeqStructA to set. |

#### Returns

a GstVC1ParserResult

### gst_vc1_parse_sequence_header_struct_b ()

    GstVC1ParserResult
    gst_vc1_parse_sequence_header_struct_b
                                   (const guint8 *data,
                                    gsize size,
                                    GstVC1SeqStructB *structb);

Parses `data` , and fills `structb` fields.

#### Parameters

data | The data to parse |
size | the size of `data` |
structb | The GstVC1SeqStructB to set. |

#### Returns

a GstVC1ParserResult

### gst_vc1_parse_sequence_header_struct_c ()

    GstVC1ParserResult
    gst_vc1_parse_sequence_header_struct_c
                                   (const guint8 *data,
                                    gsize size,
                                    GstVC1SeqStructC *structc);

Parses `data` , and fills `structc` fields.

#### Parameters

data | The data to parse |
size | the size of `data` |
structc | The GstVC1SeqStructC to set. |

#### Returns

a GstVC1ParserResult

### gst_vc1_parse_entry_point_header ()

    GstVC1ParserResult
    gst_vc1_parse_entry_point_header (const guint8 *data,
                                      gsize size,
                                      GstVC1EntryPointHdr *entrypoint,
                                      GstVC1SeqHdr *seqhdr);

Parses `data` , and sets `entrypoint` fields.

#### Parameters

data | The data to parse |
size | the size of `data` |
entrypoint | The GstVC1EntryPointHdr to set. | [out]
seqhdr | The GstVC1SeqHdr currently being parsed |

#### Returns

a GstVC1EntryPointHdr

### gst_vc1_parse_frame_header ()

    GstVC1ParserResult
    gst_vc1_parse_frame_header (const guint8 *data,
                                gsize size,
                                GstVC1FrameHdr *framehdr,
                                GstVC1SeqHdr *seqhdr,
                                GstVC1BitPlanes *bitplanes);

Parses `data` , and fills `entrypoint` fields.

#### Parameters

data | The data to parse |
size | the size of `data` |
framehdr | The GstVC1FrameHdr to fill. |
seqhdr | The GstVC1SeqHdr currently being parsed |
bitplanes | The GstVC1BitPlanes to store bitplanes in or `NULL` |

#### Returns

a GstVC1ParserResult

### gst_vc1_bitplanes_new ()

    GstVC1BitPlanes *
    gst_vc1_bitplanes_new (void);

Creates a new GstVC1BitPlanes. It should be freed with `gst_vc1_bitplanes_free()` after use.

#### Returns

a new GstVC1BitPlanes

### gst_vc1_bitplanes_free ()

    void
    gst_vc1_bitplanes_free (GstVC1BitPlanes *bitplanes);

### gst_vc1_bitplanes_free_1 ()

    void
    gst_vc1_bitplanes_free_1 (GstVC1BitPlanes *bitplanes);

### gst_vc1_bitplanes_ensure_size ()

    gboolean
    gst_vc1_bitplanes_ensure_size (GstVC1BitPlanes *bitplanes,
                                   GstVC1SeqHdr *seqhdr);

Fills the `bitplanes` structure from `seqhdr` , this function should be called after gst_vc1_parse_sequence_header if in simple or main mode, or after gst_vc1_parse_entry_point_header if in advanced mode.

#### Parameters

bitplanes | The GstVC1BitPlanes to reset |
seqhdr | The GstVC1SeqHdr from which to set `bitplanes` |

#### Returns

`TRUE` if everything went fine, `FALSE` otherwise

## Types and Values

### MAX_HRD_NUM_LEAKY_BUCKETS

    #define MAX_HRD_NUM_LEAKY_BUCKETS 31

### GST_VC1_BFRACTION_BASIS

    #define GST_VC1_BFRACTION_BASIS 840

### enum GstVC1StartCode

#### Members

GST_VC1_END_OF_SEQ |  |
GST_VC1_SLICE |  |
GST_VC1_FIELD |  |
GST_VC1_FRAME |  |
GST_VC1_ENTRYPOINT |  |
GST_VC1_SEQUENCE |  |
GST_VC1_SLICE_USER |  |
GST_VC1_FIELD_USER |  |
GST_VC1_FRAME_USER |  |
GST_VC1_ENTRY_POINT_USER |  |
GST_VC1_SEQUENCE_USER |  |

### enum GstVC1Profile

#### Members

GST_VC1_PROFILE_SIMPLE |  |
GST_VC1_PROFILE_MAIN |  |
GST_VC1_PROFILE_RESERVED |  |
GST_VC1_PROFILE_ADVANCED |  |

### enum GstVC1ParserResult

#### Members

GST_VC1_PARSER_OK |  |
GST_VC1_PARSER_BROKEN_DATA |  |
GST_VC1_PARSER_NO_BDU |  |
GST_VC1_PARSER_NO_BDU_END |  |
GST_VC1_PARSER_ERROR |  |

### enum GstVC1PictureType

#### Members

GST_VC1_PICTURE_TYPE_P |  |
GST_VC1_PICTURE_TYPE_B |  |
GST_VC1_PICTURE_TYPE_I |  |
GST_VC1_PICTURE_TYPE_BI |  |
GST_VC1_PICTURE_TYPE_SKIPPED |  |

### enum GstVC1Level

#### Members

GST_VC1_LEVEL_LOW |  |
GST_VC1_LEVEL_MEDIUM |  |
GST_VC1_LEVEL_HIGH |  |
GST_VC1_LEVEL_L0 |  |
GST_VC1_LEVEL_L1 |  |
GST_VC1_LEVEL_L2 |  |
GST_VC1_LEVEL_L3 |  |
GST_VC1_LEVEL_L4 |  |
GST_VC1_LEVEL_UNKNOWN |  |

### enum GstVC1QuantizerSpec

#### Members

GST_VC1_QUANTIZER_IMPLICITLY |  |
GST_VC1_QUANTIZER_EXPLICITLY |  |
GST_VC1_QUANTIZER_NON_UNIFORM |  |
GST_VC1_QUANTIZER_UNIFORM |  |

### enum GstVC1DQProfile

#### Members

GST_VC1_DQPROFILE_FOUR_EDGES |  |
GST_VC1_DQPROFILE_DOUBLE_EDGES |  |
GST_VC1_DQPROFILE_SINGLE_EDGE |  |
GST_VC1_DQPROFILE_ALL_MBS |  |

### enum GstVC1Condover

#### Members

GST_VC1_CONDOVER_NONE |  |
GST_VC1_CONDOVER_ALL |  |
GST_VC1_CONDOVER_SELECT |  |

### enum GstVC1MvMode

#### Members

GST_VC1_MVMODE_1MV_HPEL_BILINEAR |  |
GST_VC1_MVMODE_1MV |  |
GST_VC1_MVMODE_1MV_HPEL |  |
GST_VC1_MVMODE_MIXED_MV |  |
GST_VC1_MVMODE_INTENSITY_COMP |  |

### struct GstVC1SeqHdr

    struct GstVC1SeqHdr {
      GstVC1Profile profile;

      GstVC1SeqStructC struct_c;

      /*  calculated */
      guint mb_height;
      guint mb_width;
      guint mb_stride;

      GstVC1AdvancedSeqHdr   advanced;
    };

Structure for sequence headers in any profile.

### struct GstVC1AdvancedSeqHdr

    struct GstVC1AdvancedSeqHdr {
      GstVC1Level  level;

      guint8  frmrtq_postproc;
      guint8  bitrtq_postproc;
      guint8  postprocflag;
      guint16 max_coded_width;
      guint16 max_coded_height;
      guint8  pulldown;
      guint8  interlace;
      guint8  tfcntrflag;
      guint8  finterpflag;
      guint8  psf;
      guint8  display_ext;
      guint16 disp_horiz_size;
      guint16 disp_vert_size;
      guint8  aspect_ratio_flag;
      guint8  aspect_ratio;
      guint8  aspect_horiz_size;
      guint8  aspect_vert_size;
      guint8  framerate_flag;
      guint8  framerateind;
      guint8  frameratenr;
      guint8  frameratedr;
      guint16 framerateexp;
      guint8  color_format_flag;
      guint8  color_prim;
      guint8  transfer_char;
      guint8  matrix_coef;
      guint8  hrd_param_flag;
      guint8  colordiff_format;

      GstVC1HrdParam hrd_param;

      /* computed */
      guint framerate; /* Around in fps, 0 if unknown*/
      guint bitrate;   /* Around in kpbs, 0 if unknown*/
      guint par_n;
      guint par_d;
      guint fps_n;
      guint fps_d;

      /* The last parsed entry point */
      GstVC1EntryPointHdr entrypoint;
    };

Structure for the advanced profile sequence headers specific parameters.

### struct GstVC1SeqLayer

    struct GstVC1SeqLayer {
      guint32 numframes;

      GstVC1SeqStructA struct_a;
      GstVC1SeqStructB struct_b;
      GstVC1SeqStructC struct_c;
    };

### struct GstVC1SeqStructA

    struct GstVC1SeqStructA {
      guint32 vert_size;
      guint32 horiz_size;
    };

### struct GstVC1SeqStructB

    struct GstVC1SeqStructB {
      GstVC1Level  level;

      guint8 cbr;
      guint32 framerate;

      /* In simple and main profiles only */
      guint32 hrd_buffer;
      guint32 hrd_rate;
    };

### struct GstVC1SeqStructC

    struct GstVC1SeqStructC {
      GstVC1Profile profile;

      /* Only in simple and main profiles */
      guint8 frmrtq_postproc;
      guint8 bitrtq_postproc;
      guint8 res_sprite;
      guint8 loop_filter;
      guint8 multires;
      guint8 fastuvmc;
      guint8 extended_mv;
      guint8 dquant;
      guint8 vstransform;
      guint8 overlap;
      guint8 syncmarker;
      guint8 rangered;
      guint8 maxbframes;
      guint8 quantizer;
      guint8 finterpflag;

      /* Computed */
      guint framerate; /* Around in fps, 0 if unknown*/
      guint bitrate;   /* Around in kpbs, 0 if unknown*/

      /* This should be filled by user if previously known */
      guint16 coded_width;
      /* This should be filled by user if previously known */
      guint16 coded_height;

      /* Wmvp specific */
      guint8 wmvp;          /* Specify if the stream is wmp or not */
      /* In the wmvp case, the framerate is not computed but in the bistream */
      guint8 slice_code;
    };

### struct GstVC1HrdParam

    struct GstVC1HrdParam {
      guint8 hrd_num_leaky_buckets;
      guint8 bit_rate_exponent;
      guint8 buffer_size_exponent;
      guint16 hrd_rate[MAX_HRD_NUM_LEAKY_BUCKETS];
      guint16 hrd_buffer[MAX_HRD_NUM_LEAKY_BUCKETS];
    };

### struct GstVC1EntryPointHdr

    struct GstVC1EntryPointHdr {
      guint8 broken_link;
      guint8 closed_entry;
      guint8 panscan_flag;
      guint8 refdist_flag;
      guint8 loopfilter;
      guint8 fastuvmc;
      guint8 extended_mv;
      guint8 dquant;
      guint8 vstransform;
      guint8 overlap;
      guint8 quantizer;
      guint8 coded_size_flag;
      guint16 coded_width;
      guint16 coded_height;
      guint8 extended_dmv;
      guint8 range_mapy_flag;
      guint8 range_mapy;
      guint8 range_mapuv_flag;
      guint8 range_mapuv;

      guint8 hrd_full[MAX_HRD_NUM_LEAKY_BUCKETS];
    };

Structure for entrypoint header, this will be used only in advanced profiles

### struct GstVC1FrameHdr

    struct GstVC1FrameHdr {
      /* common fields */
      GstVC1PictureType ptype;
      guint8 interpfrm;
      guint8 halfqp;
      guint8 transacfrm;
      guint8 transdctab;
      guint8 pqindex;
      guint8 pquantizer;

      /* Computed */
      guint8 pquant;

      /* Convenience fields */
      guint8 profile;
      guint8 dquant;

      /*  If dquant */
      GstVC1VopDquant vopdquant;

      union {
        GstVC1PicSimpleMain simple;
        GstVC1PicAdvanced advanced;
      } pic;

      /* Size of the picture layer in bits */
      guint header_size;
    };

Structure that represent picture in any profile or mode. You should look at `ptype` and `profile` to know what is currently in use.

### struct GstVC1PicAdvanced

    struct GstVC1PicAdvanced {
      GstVC1FrameCodingMode fcm;
      guint8  tfcntr;

      guint8  rptfrm;
      guint8  tff;
      guint8  rff;
      guint8  ps_present;
      guint32 ps_hoffset;
      guint32 ps_voffset;
      guint16 ps_width;
      guint16 ps_height;
      guint8  rndctrl;
      guint8  uvsamp;
      guint8  postproc;

      /*  B and P picture specific */
      guint8  mvrange;
      guint8  mvmode;
      guint8  mvtab;
      guint8  cbptab;
      guint8  ttmbf;
      guint8  ttfrm;

      /* B and BI picture only
       * Should be divided by #GST_VC1_BFRACTION_BASIS
       * to get the real value. */
      guint16 bfraction;

      /* ppic */
      guint8  mvmode2;
      guint8  lumscale;
      guint8  lumshift;

      /* bipic */
      guint8  bf;
      guint8  condover;
      guint8  transacfrm2;

      /* Biplane value, those fields only mention the fact
       * that the bitplane is in raw mode or not */
      guint8  acpred;
      guint8  overflags;
      guint8  mvtypemb;
      guint8  skipmb;
      guint8  directmb;
      guint8  forwardmb; /* B pic interlace field only */

      /* For interlaced pictures only */
      guint8  fieldtx;

      /* P and B pictures */
      guint8  intcomp;
      guint8  dmvrange;
      guint8  mbmodetab;
      guint8  imvtab;
      guint8  icbptab;
      guint8  mvbptab2;
      guint8  mvbptab4; /* If 4mvswitch in ppic */

      /*  P picture */
      guint8  mvswitch4;

      /* For interlaced fields only */
      guint16 refdist;
      guint8 fptype; /* Raw value */

      /* P pic */
      guint8  numref;
      guint8  reffield;
      guint8  lumscale2;
      guint8  lumshift2;
      guint8  intcompfield;
    };

#### Members

GstVC1FrameCodingMode `fcm`; |  |
guint8 `tfcntr`; |  |
guint8 `rptfrm`; |  |
guint8 `tff`; |  |
guint8 `rff`; |  |
guint8 `ps_present`; |  |
guint32 `ps_hoffset`; |  |
guint32 `ps_voffset`; |  |
guint16 `ps_width`; |  |
guint16 `ps_height`; |  |
guint8 `rndctrl`; |  |
guint8 `uvsamp`; |  |
guint8 `postproc`; |  |
guint8 `mvrange`; |  |
guint8 `mvmode`; |  |
guint8 `mvtab`; |  |
guint8 `cbptab`; |  |
guint8 `ttmbf`; |  |
guint8 `ttfrm`; |  |
guint16 `bfraction`; |  |
guint8 `mvmode2`; |  |
guint8 `lumscale`; |  |
guint8 `lumshift`; |  |
guint8 `bf`; |  |
guint8 `condover`; |  |
guint8 `transacfrm2`; |  |
guint8 `acpred`; |  |
guint8 `overflags`; |  |
guint8 `mvtypemb`; |  |
guint8 `skipmb`; |  |
guint8 `directmb`; |  |
guint8 `forwardmb`; |  |
guint8 `fieldtx`; |  |
guint8 `intcomp`; |  |
guint8 `dmvrange`; |  |
guint8 `mbmodetab`; |  |
guint8 `imvtab`; |  |
guint8 `icbptab`; |  |
guint8 `mvbptab2`; |  |
guint8 `mvbptab4`; |  |
guint8 `mvswitch4`; |  |
guint16 `refdist`; |  |
guint8 `fptype`; |  |
guint8 `numref`; |  |
guint8 `reffield`; |  |
guint8 `lumscale2`; |  |
guint8 `lumshift2`; |  |
guint8 `intcompfield`; |  |

### struct GstVC1PicSimpleMain

    struct GstVC1PicSimpleMain {
      guint8 frmcnt;
      guint8 mvrange;
      guint8 rangeredfrm;

      /* I and P pic simple and main profiles only */
      guint8 respic;

      /* I and BI pic simple and main profiles only */
      guint8 transacfrm2;
      guint8 bf;

      /* B and P pic simple and main profiles only */
      guint8 mvmode;
      guint8 mvtab;
      guint8 ttmbf;

      /* P pic simple and main profiles only */
      guint8 mvmode2;
      guint8 lumscale;
      guint8 lumshift;

      guint8 cbptab;
      guint8 ttfrm;

      /* B and BI picture only
       * Should be divided by #GST_VC1_BFRACTION_BASIS
       * to get the real value. */
      guint16 bfraction;

      /* Biplane value, those fields only mention the fact
       * that the bitplane is in raw mode or not */
      guint8 mvtypemb;
      guint8 skipmb;
      guint8 directmb; /* B pic main profile only */
    };

#### Members

guint8 `frmcnt`; |  |
guint8 `mvrange`; |  |
guint8 `rangeredfrm`; |  |
guint8 `respic`; |  |
guint8 `transacfrm2`; |  |
guint8 `bf`; |  |
guint8 `mvmode`; |  |
guint8 `mvtab`; |  |
guint8 `ttmbf`; |  |
guint8 `mvmode2`; |  |
guint8 `lumscale`; |  |
guint8 `lumshift`; |  |
guint8 `cbptab`; |  |
guint8 `ttfrm`; |  |
guint16 `bfraction`; |  |
guint8 `mvtypemb`; |  |
guint8 `skipmb`; |  |
guint8 `directmb`; |  |

### GstVC1Picture

    typedef struct _GstVC1Picture GstVC1Picture;

### struct GstVC1VopDquant

    struct GstVC1VopDquant {
      guint8 pqdiff;
      guint8 abspq;

      /* Computed */
      guint8 altpquant;

      /*  if dqant != 2*/
      guint8 dquantfrm;
      guint8 dqprofile;

      /* Boundary edge selection. This represents DQSBEDGE
       * if dqprofile == GST_VC1_DQPROFILE_SINGLE_EDGE or
       * DQDBEDGE if dqprofile == GST_VC1_DQPROFILE_DOUBLE_EDGE */
      guint8 dqbedge;

      /* FIXME: remove */
      guint8 unused;

      /* if dqprofile == GST_VC1_DQPROFILE_ALL_MBS */
      guint8 dqbilevel;
    };

### struct GstVC1BDU

    struct GstVC1BDU {
      GstVC1StartCode type;
      guint size;
      guint sc_offset;
      guint offset;
      guint8 * data;
    };

Structure that represents a Bitstream Data Unit.