## intervideosrc intervideosrc |

## Properties

gchar * | channel | Read / Write
guint64 | timeout | Read / Write

## Types and Values

struct | GstInterVideoSrc

## Object Hierarchy

        GObject
        ╰── GInitiallyUnowned
            ╰── GstObject
                ╰── GstElement
                    ╰── GstBaseSrc
                        ╰── GstInterVideoSrc

## Description

## Synopsis

### Element Information

plugin | inter
author | David Schleef <ds@schleef.org>
class | Source/Video

### Element Pads

name | src
direction | source
presence | always
details | video/x-raw, format=(string){ I420, YV12, YUY2, UYVY, AYUV, VUYA, RGBx, BGRx, xRGB, xBGR, RGBA, BGRA, ARGB, ABGR, RGB, BGR, Y41B, Y42B, YVYU, Y444, v210, v216, Y210, Y410, NV12, NV21, GRAY8, GRAY16_BE, GRAY16_LE, v308, RGB16, BGR16, RGB15, BGR15, UYVP, A420, RGB8P, YUV9, YVU9, IYU1, ARGB64, AYUV64, r210, I420_10BE, I420_10LE, I422_10BE, I422_10LE, Y444_10BE, Y444_10LE, GBR, GBR_10BE, GBR_10LE, NV16, NV24, NV12_64Z32, A420_10BE, A420_10LE, A422_10BE, A422_10LE, A444_10BE, A444_10LE, NV61, P010_10BE, P010_10LE, IYU2, VYUY, GBRA, GBRA_10BE, GBRA_10LE, BGR10A2_LE, GBR_12BE, GBR_12LE, GBRA_12BE, GBRA_12LE, I420_12BE, I420_12LE, I422_12BE, I422_12LE, Y444_12BE, Y444_12LE, GRAY10_LE32, NV12_10LE32, NV16_10LE32, NV12_10LE40 }, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 0/1, 2147483647/1 ]

## Functions

## Types and Values

### struct GstInterVideoSrc

    struct GstInterVideoSrc;

## Property Details

### The `“channel”` property

      “channel”                  gchar *

Channel name to match inter src and sink elements.

Flags: Read / Write

Default value: "default"

### The `“timeout”` property

      “timeout”                  guint64

Timeout after which to start outputting black frames.

Flags: Read / Write

Default value: 1000000000