## dc1394src dc1394src |

## Properties

guint | dma | Read / Write
gchar * | guid | Read / Write
GstDC1394ISOSpeed | iso | Read / Write
gint | unit | Read / Write

## Types and Values

struct | GstDC1394Src

## Object Hierarchy

        GObject
        ╰── GInitiallyUnowned
            ╰── GstObject
                ╰── GstElement
                    ╰── GstBaseSrc
                        ╰── GstPushSrc
                            ╰── GstDC1394Src

## Description

Source for IIDC (Instrumentation & Industrial Digital Camera) firewire cameras. If several cameras are connected to the system, the desired one can be selected by its GUID and an optional unit number (most cameras are single unit and do not require it). The frame size, rate and format are set from capabilities. Although the IIDC specification includes a raw video mode, many cameras use mono video modes to capture in Bayer format. Thus, for each mono video mode supported by a camera, both gray raw and Bayer corresponding video formats are exposed in the capabilities. The Bayer pattern is left unspecified.

#### Example launch lines

    1
    gst-launch-1.0 -v dc1394src ! videoconvert ! autovideosink

Capture and display frames from the first camera available in the system.

    1
    2
    3
    gst-launch-1.0 dc1394src guid=00074813004DF937 \
        ! "video/x-bayer,format=gbrg,width=1280,height=960,framerate=15/2" \
        ! bayer2rgb ! videoconvert ! autovideosink

Capture and display frames from a specific camera in the desired format.

## Synopsis

### Element Information

plugin | dc1394
author | Antoine Tremblay <hexa00@gmail.com>
class | Source/Video

### Element Pads

name | src
direction | source
presence | always
details | video/x-raw, format=(string)IYU2, width=(int)160, height=(int)120, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)UYVY, width=(int)320, height=(int)240, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)IYU1, width=(int)640, height=(int)480, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)UYVY, width=(int)640, height=(int)480, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)RGB, width=(int)640, height=(int)480, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)GRAY8, width=(int)640, height=(int)480, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-bayer, format=(string){ bggr, rggb, grbg, gbrg }, width=(int)640, height=(int)480, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)GRAY16_BE, width=(int)640, height=(int)480, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)UYVY, width=(int)800, height=(int)600, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)RGB, width=(int)800, height=(int)600, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)GRAY8, width=(int)800, height=(int)600, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-bayer, format=(string){ bggr, rggb, grbg, gbrg }, width=(int)800, height=(int)600, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)UYVY, width=(int)1024, height=(int)768, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)RGB, width=(int)1024, height=(int)768, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)GRAY8, width=(int)1024, height=(int)768, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-bayer, format=(string){ bggr, rggb, grbg, gbrg }, width=(int)1024, height=(int)768, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)GRAY16_BE, width=(int)800, height=(int)600, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)GRAY16_BE, width=(int)1024, height=(int)768, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)UYVY, width=(int)1280, height=(int)960, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)RGB, width=(int)1280, height=(int)960, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)GRAY8, width=(int)1280, height=(int)960, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-bayer, format=(string){ bggr, rggb, grbg, gbrg }, width=(int)1280, height=(int)960, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)UYVY, width=(int)1600, height=(int)1200, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)RGB, width=(int)1600, height=(int)1200, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)GRAY8, width=(int)1600, height=(int)1200, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-bayer, format=(string){ bggr, rggb, grbg, gbrg }, width=(int)1600, height=(int)1200, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)GRAY16_BE, width=(int)1280, height=(int)960, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)GRAY16_BE, width=(int)1600, height=(int)1200, framerate=(fraction){ 15/8, 15/4, 15/2, 15/1, 30/1, 60/1, 120/1, 240/1 }
| video/x-raw, format=(string)RGB, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 1/2147483647, 2147483647/1 ]
| video/x-raw, format=(string)IYU2, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 1/2147483647, 2147483647/1 ]
| video/x-raw, format=(string)UYVY, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 1/2147483647, 2147483647/1 ]
| video/x-raw, format=(string)IYU1, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 1/2147483647, 2147483647/1 ]
| video/x-raw, format=(string)GRAY16_BE, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 1/2147483647, 2147483647/1 ]
| video/x-bayer, format=(string){ bggr, rggb, grbg, gbrg }, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 1/2147483647, 2147483647/1 ]
| video/x-raw, format=(string)GRAY8, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 1/2147483647, 2147483647/1 ]
| video/x-bayer, format=(string){ bggr, rggb, grbg, gbrg }, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 1/2147483647, 2147483647/1 ]

## Functions

## Types and Values

### struct GstDC1394Src

    struct GstDC1394Src;

## Property Details

### The `“dma”` property

      “dma”                      guint

The number of frames in the Direct Memory Access ring buffer.

Flags: Read / Write

Allowed values: >= 1

Default value: 10

### The `“guid”` property

      “guid”                     gchar *

The hexadecimal representation of the GUID of the camera (use first camera available if null).

Flags: Read / Write

Default value: NULL

### The `“iso”` property

      “iso”                      GstDC1394ISOSpeed

The ISO bandwidth in Mbps.

Flags: Read / Write

Default value: DC1394 ISO speed 400

### The `“unit”` property

      “unit”                     gint

The unit number of the camera (-1 if no unit number is used).

Flags: Read / Write

Allowed values: >= G_MAXULONG

Default value: -1